Real-Time Sonar Beamformingon a Unix Workstation usingProcess Networks and POSIX PthreadsGregory E. Allen

24 February 1998

Motivation¥ Beamforming is a computationally intense algorithm which has traditionally been limited to expensive custom hardware. (GFLOPS)¥ Current multi-processor RISC workstations post benchmarks that approach these capabilities at a fraction of the cost.¥ Real-time performance has traditionally been beyond the capabilities of standard Unix.¥ POSIX Real-time extensions (including Pthreads) with symmetric multiprocessing could allow a workstation implementation.

Objectives¥ Utilize the process networks model, which is a natural way to describe signal processing systems.¥ Implement high-performance, low-overhead process networks using lightweight threads.¥ Implement and benchmark �digital interpolated beamformer� algorithms.¥ Create a real-time beamformer on a workstation that can replace custom hardware.

Implementation¥ Used Matlab to generate and test beam coefficients, and to verify beamformer output.¥ Developed C++ code to implement process networks and digital interpolated beamforming.¥ Used existing Pthread and timer classes.¥ Developed a Process Network queue class.¥ Developed a sparse FIR filter (using coefficients from Matlab).¥ Developed other (more optimized) beamforming kernels.

¥ Developed several different beamforming implementations for comparison.

Process Networks Queue Class

Each process is a POSIX thread, and UNIX does the scheduling.

Use Parks� rules for dynamic scheduling of process networks:

A processes blocks if it reads from an empty queue.

A process blocks if it writes to a full queue.

(We assume that queues are large enough to avoid artificial deadlock, and that the program is not unbounded.)

Borrow the idea of a firing threshold (Tp) from Karp and Miller.

Queue threshold is max[ Up, Wp, Tp ].

Intended to be optimized for DSP applications:

Processes operate directly from queue memory, so that no data has to be copied.

Data is guaranteed to be contiguous in memory to make up for the lack of circular addressing modes on a general-purpose processor.

There is a tradeoff between memory usage and performance.

Beamforming Implementations

¥ Batch-mode, with a single thread of execution.

¥ Batch-mode, with multiple threads of execution.

¥ Process Network, with a single thread beamformer.

¥ Process Network, with a multi-threaded beamformer.¥ Multiple threads divide the task of calculation.

¥ How the task is divided can greatly affect the performance.¥ Multiple threads divide the task of calculation.

¥ �Thread pools� -- merging DSP and workstation algorithms.¥ All sensor data is read into memory.¥ One task calculates results from memory to memory.

¥ All results are written out to disk.¥ A producer thread and a consumer thread provide an interface from memory to Process Network queues.¥ A beamforming thread takes samples from the producer, calculates the result, and sends it to the consumer.

Dividing The Beamforming Job

¥ Divide by beams

¥ Divide by samples

¥ Tips for performance.¥�Partial Beamforming�.¥Low latency.¥Low memory use.¥Poor cache utilization.¥

A �DSP� approach¥Good cache utilization.¥Higher latency.¥More memory usage.¥

A �workstation� approach.

<-beams->

<-samples->

¥These are DSP algorithms, but they are running on a workstation.¥Throughput is more importatant than memory usage or latency.¥

Keep each thread�s kernel calculations in the cache.

Results¥Used average time over 10 trials to calculate 10000 beam sets.¥All cases divided computation by samples, for best performance.¥Benchmarks performed on a Sun Ultra-2 workstation with dual 300 MHz UltraSPARC-II CPUs.¥4 CPU benchmarks performed on a Sun SPARCserver 670MP workstation with quad

72 MHz HyperSPARC CPUs.

Comments¥ Kernel performance of about 19,000 samples per second per CPU.¥33% overhead for process networks.¥

Process network overhead is inflated because of data copying.

Batch-mode

Process network

Beamformer typeSeconds

1 CPU

0.270

0.360Seconds

2 CPUs

Speedup

4 CPUs

97%90%290%

210%

0.532

0.682

Expected Current Performance¥The Process Networks queue has been rewritten for better memory-to-memory operation, which should substantially boost performance and reduce overhead. Previously, only consumers operated out of queue memory.¥Beamformer kernel (batch mode) routines have reached upwards of 35,000 samples per second per CPU (better than 80% speedup).¥Advanced Sonar Group (ASG) just installed a quad 300 MHz UltraSPARC-II workstation, and is ordering a workstation with

8 UltraSPARC-II CPUs running at 333 MHz.

Conclusion¥Realization of a real-time beamformer on a Unix workstation is on the horizon.¥A workstation beamformer could be implemented at a fraction of the cost of custom hardware.¥ As workstations become even faster, custom hardware beamformers may become obsolete.

Future Work¥ A three-fan vertical beamformer with 3 digital interpolation

(horizontal) beamformers. Current estimate, 16 to 20 CPUs.

¥ An entire real-time sonar on a workstation?

sensor datasensor data40 MB/sec eachThree-fanVertical

Beamformer32 MB/sec eachDigitalInterpolation

BeamformerDigitalInterpolation

Beamformer complex band shift downsample by 824 MB/sec each6 MB/sec eachcomplex by 8complex by 848 MB/sec each